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Release Notes AP72W_1.0.58.10


1. Release Overview
	Product
	WS-AP72W

	Version
	AP72W_1.0.58.10

	Release Date
	2026-09-18

	Build ID
	

	Release Type
	GA

	Upgrade Recommendation
	Recommended


2. Supported Platforms
· All hardware versions of WS-AP72W are supported
3. Key Highlights
· [bookmark: _GoBack]Fixed known bugs and resolved the issue where the AP works abnormally under certain scenarios
4. New Features
· None
5. Enhancements
· None
6. Bug Fixes
· Fixed the issue where the WiFi radio was disabled when the gateway was unreachable via ping
· Fixed the issue where, after the TV entered sleep mode, AP waking up the STA caused it to wake up.
· Fixed the issue where the AP failed to connect to the AC when the AP and AC were assigned to different subnets.
7. Known Issues
- None.
8. Compatibility & Dependencies
· Compatible AC versions
	Unify AC
	UnifyAC_CR_1.0.6.3 or later


9. Upgrade Instructions
- Upgrade from Unify AC at UnifyAC_CR_1.0.6.3 or later

Notes:
- Downtime: lower than 5 minutes (single)
- Config retained: Yes
10. Downgrade / Rollback
- Supported version: AP72W_1.0.44 or later
- Config compatibility: Full
11. TAC Advisory
- Recommended upgrade scenarios: All deployments
- Known risks in previous versions: 
12. Deployment Notes
- Suitable for standard managed WiFi scenarios
13. PoE Power Budget
- Optical-electrical Hybrid Cable or DC Power Supply Scenario (with 100watts PSU)
     Dual PSE Port can supports up to 30W Power out.
- PoE Power Supply Scenario
     One PSE Port can supports up to 10W Power out, do not use two PSE ports simultaneously .
14. Thermal Advisory
- Passive Heat Dissipation, do not cover the surface with any objects
15. Security Updates
Not applicable
16. Documentation & Support
- Support: support@westalatech.com
17. Disclaimer
- Westala reserves the right to modify specifications without notice.
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